For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the rear compartment lid in order to access the tail lamp screws.

1 | Tail Lamp Assembly Screws (Qty: 2) Tighten 2.5 N·m (22 lb in)
2 | Chassis Electrical Connector Procedure Lift the tail lamp in order to disengage the retainer clips then disconnect the electrical connector.
3 | Tail Lamp Assembly Tip Transfer the bulb into the new tail lamp.
4 | Quarter Filler Panel Nuts (Qty: 2) Tip Ensure the quarter filler panel nuts are not damaged. Replace if damaged.