For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the tires and wheels. Refer to Tire and Wheel Removal and Installation .
2. Separate the rear adjustment link from the suspension knuckle. DO NOT loosen the adjustment jamb nut. Refer to Adjust Link Replacement .

1 | Upper Shock Module Mounting Nut (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 47 N·m (35 lb ft)
2 | Lower Shock Module Mounting Nut (Qty: 2) Tighten 28 N·m (21 lb ft)
3 | Lower Shock Module Mounting Bolt
4 | Shock Module Tip Remove the shock module toward the rear of the vehicle.