For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Disconnect the shift linkage from the shift control. Refer to Shift Control Linkage Replacement .
3. Lower the vehicle.
4. Remove the shift indicator and shift knob assembly. Refer to Transmission Control Lever Knob Replacement .
5. Remove the instrument panel (I/P) center support bracket. Refer to Instrument Panel Center Support Bracket Replacement .

1 | Shift Control Rivet (Qty: 5)
2 | Shift Control