For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
2. Drain the washer solvent into a suitable clean container.

1 | Windshield Washer Pump Hose Assembly Procedure

1. Disconnect the hose at the hinge pillar and air inlet panel.
2. Disengage the integral washer hose clip from the electronic control module (ECM) bracket.

2 | Windshield Washer Solvent Container Screws (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
3 | Windshield Washer Container Assembly Tip Lower the windshield washer container from behind the left front fender area.
4 | Windshield Washer Container Pump Kit Procedure Disconnect the washer hose at the pump and use two flat-bladed tools and pry the washer pump from the container.