For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. With the park brake lever fully released, completely back off the adjustment nut.

The park brake cable adjusting nut is a nylon lock type. Use ONLY HAND TOOLS whenever tightening or loosening the adjusting nut.

3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Remove the rear tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation .

1 | Park Brake Cable Equalizer

#### Procedure

1. Carefully position the driveline tunnel insulator downward just enough to access the cable equalizer.
2. Rotate the front cable end to release the cable from the equalizer.

2 | Park Brake Cable

#### Procedure

1. Release the wheel speed sensor harness clips from the park brake cable.
2. Disconnect the park brake cables from the park brake actuator levers on the brake calipers.

3 | Park Brake Cable Retainer (Qty: 2)
4 | Park Brake Cable Assembly

#### Procedure

Move the cable conduit rearward to clear the tunnel bracket, then lift the cables to release the cables from the bracket.