For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the radiator outlet hose. Refer to Radiator Outlet Hose Replacement.

1 | Power Steering Gear Outlet Hose Fitting Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Place drain pans under the vehicle as needed to catch any power steering fluid.

Tighten
27 N·m (20 lb ft)

2 | Power Steering Gear Outlet Hose Bracket Bolt (Qty: 2) Tighten 9 N·m (80 lb in)
3 | Power Steering Gear Outlet Hose Clip (Qty: 2)
4 | Power Steering Gear Outlet Hose

#### Procedure

1. Remove the power steering gear outlet hose clamp.
2. Fill and bleed the power steering system. Refer to Power Steering System Bleeding.

5 | Power Steering Gear Inlet Hose Fitting

#### Procedure

Place drain pans under the vehicle as needed to catch any power steering fluid.

Tighten
27 N·m (20 lb ft)

6 | Power Steering Gear Inlet Hose Fitting

#### Procedure

Place drain pans under the vehicle as needed to catch any power steering fluid.

Tighten
27 N·m (20 lb ft)

7 | Power Steering Gear Inlet Hose

#### Procedure

Fill and bleed the power steering system. Refer to Power Steering System Bleeding.