For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Slide front seats forward and tilt seat back down.
2. Remove door sill trim. Refer to Door Sill Plate Replacement.
3. Remove lock pillar trim panel. Refer to Body Lock Pillar Trim Panel Replacement.
4. Remove the rear window panel trim. Refer to Rear Window Panel Trim Replacement.
5. Remove the front side door rear weatherstrip. Refer to Front Side Door Rear Weatherstrip Replacement.

1 | Rear Compartment Front Trim Panel Screw (Qty: 16) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear Compartment Front Trim Panel Assembly