For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Assembly

#### Procedure

1. Depress the outboard tabs securing the lamp assembly to the rear bumper fascia.
2. Swing the lamp assembly downward.
3. Disconnect the electrical connector.

2 | Rear License Plate Lamp Socket

#### Procedure

1. Twist the lamp socket counterclockwise in order to remove from the lamp housing.
2. Replace the bulb, as needed.