For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Unlatch the folding top and position the No. 1 bow in the upright position.

1 | Folding Top Front Handle Cover Tip The replacement latch does not include the handle. The handle will need to be transferred over from the original latch.
2 | Folding Top Front Handle Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 21 N·m (16 lb ft)
3 | Folding Top Front Handle
4 | Folding Top Front Latch Screw (Qty: 3) Tip The screws can be accessed for removal between the No. 1 bow and the folding top cover. Tighten 9 N·m (80 lb in)
5 | Folding Top Front Latch