For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement .

1 | Instrument Panel Compartment Frame Bolt Caps (Qty: 2)
2 | Instrument Panel Compartment Frame Bolts (Qty: 5) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
3 | Instrument Panel Compartment Frame Screws (Qty: 2) Tighten 2.5 N·m (22 lb in)
4 | Instrument Panel Compartment Frame Assembly

#### Procedures

1. Disconnect the electrical connections.
2. When replacing the compartment frame assembly, transfer all necessary components.