For 1990-2009 cars

#### Special Tools

EL-39200 Digital Multimeter

For equivalent regional tools, refer to Special Tools.

Notice: Refer to Test Probe Notice in the Preface section.

Note: Circuits which include any solid state control modules, such as the powertrain control module (PCM), should only be tested with a 10 MΩ or higher impedance digital multimeter such as the EL-39200 Digital Multimeter (DMM).

The EL-39200 instruction manual is a good source of information and should be read thoroughly upon receipt of the DMM as well as kept on hand for future reference.

A DMM should be used instead of a test lamp in order to test for voltage in high impedance circuits. While a test lamp shows whether voltage is present if the impedance is low enough, a DMM indicates how much voltage is present. In other words, if there is not enough current, the test lamp will not illuminate even though voltage is present.

The ohmmeter function on a DMM shows how much resistance exists between 2 points along a circuit. Low resistance in a circuit means good continuity.

Note: Disconnect the power feed from the suspect circuit when measuring resistance with a DMM. This prevents incorrect readings. DMMs apply such a small voltage to measure resistance that the presence of voltages can upset a resistance reading.

Diodes and solid state components in a circuit can cause a DMM to display a false reading. To find out if a component is affecting a measurement take a reading once, then reverse the leads and take a second reading. If the readings differ the solid state component is affecting the measurement.

Following are examples of the various methods of connecting the DMM to the circuit to be tested:

• | Backprobe both ends of the connector and either hold the leads in place while manipulating the connector or tape the leads to the harness for continuous monitoring while you perform other operations or test driving. Refer to Probing Electrical Connectors.

• | Disconnect the harness at both ends of the suspected circuit where it connects either to a component or to other harnesses.

• | If the system that is being diagnosed has a specified pinout or breakout box, it may be used in order to simplify connecting the DMM to the circuit or for testing multiple circuits quickly.