For 1990-2009 cars

## Rear Bumper Fascia Molding Replacement LWB

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
3. Remove the rear bumper fascia rub-strip to rear bumper fascia retaining clips (1).
4. Remove the rear bumper fascia rub-strip from the rear bumper fascia.

### Installation Procedure

1. Install the rear bumper fascia rub-strip to rear bumper fascia.
2. Install the rear bumper fascia rub-strip to rear bumper fascia retaining clips (1).
3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
4. Lower the vehicle.