For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the transmission fluid pan and filter. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement .
3. Remove the upper and lower valve body assembly. Refer to Control Valve Lower Body and Upper Body Replacement .

1 | Speed Sensor Electrical Connector
2 | Input and Output Speed Sensor Assembly Bolts (Qty: 2) Tighten 12 N·m (106 lb. in)
3 | Input and Output Speed Sensor Assembly Clips (Qty: 2) Tip Inspect the wiring harness clips for damage replace if necessary.
4 | Input and Output Speed Sensor Assembly