For 1990-2009 cars

## 2-6 Clutch Backing Plate Retaining Ring Measurement 6L50

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Install DT 47868-1 clutch pack travel weight and DT-47868-4 travel weight adapter onto the 2-6 clutch backing plate.
2. Attach the J 8001 dial indicator set to the J 26900-13 magnetic base and zero out the dial indicator on the DT 47868-1 clutch pack travel weight .

#### Special Tools

• | DT 47868-1 Clutch Pack Travel Weight

• | DT-47868-4 Clutch Travel Weight Adapter

• | J 8001 Dial Indicator Set

• | J 26900-13 Magnetic Base

For equivalent regional tools, refer to Special Tools.

1 | 2-6 Clutch Apply Passage Tip Apply compressed air to the apply passage hole, at least 3 times and observe the dial indicator measurement each time. This action "fluffs" the clutch plates to ensure an accurate measurement. Refer to Clutch Backing Plate Retaining Ring Specifications.