For 1990-2009 cars

Replace the wheel if any of the following conditions exist:

• | The wheel exhibits excessive runout.

• | The wheel is bent.

• | The wheel mounting surface is bent.

• | The wheel is cracked.

• | The wheel is severely rusted.

• | The wheel is severely corroded.

Replace the wheel, the wheel hub studs and the wheel nuts, if any of the following conditions exist:

• | The wheel has elongated wheel stud holes.

• | The wheel nuts loosen repeatedly.

Caution: Refer to General Repair Instructions in the Preface section.

Notice: Refer to General Repair Instructions in the Preface section.

Important:

• | Replacement wheels must be equivalent to the original equipment wheels in the following ways:

- | The load capacity.

- | The wheel diameter.

- | The rim width.

- | The wheel offset.

- | The mounting configuration.

• | A wheel of the incorrect size or type may affect the following conditions:

- | Wheel and hub-bearing life.

- | Brake cooling.

- | Speedometer/odometer calibration.

- | Vehicle ground clearance.

- | Tire clearance to the body and the chassis.

Steel wheel identification is stamped into the wheel rim.

Aluminium wheel identification is cast into the inboard side of the wheel.