For 1990-2009 cars

### Removal Procedure

1. Raise the window to the full up position.
2. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement.
3. Pull the rear half of the water deflector away from the door panel in order to access the door latch.

Important: Pry the outside door handle rod retaining clip (1) using a suitable tool.

4. Disconnect the outside door handle rod (1) from the door latch (2).
5. Disconnect the door latch electrical connector (1).

Important: The door latch to door retaining screws (2) are single use parts and must be discarded after use.

Important: Support the door latch when removing the door latch retaining screws (1).

6. Remove the door latch to door retaining screws (1).

Discard the screws.

Important: Remove the door latch through the door cavity.

7. Remove the door latch from the door with the inside door handle cable and inside door lock cable attached.
8. Disconnect the inside door handle cable and inside door lock cable from the door latch. Refer to Rear Side Door Inside Handle Cable Replacement.

### Installation Procedure

1. Connect the inside door handle cable and inside door lock cable to the door latch. Refer to Rear Side Door Inside Handle Cable Replacement.

Important: Position the door latch through the door cavity and support. .

2. Position the door latch into the door.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the door latch to door NEW retaining screws (1).

Tighten
Tighten the screws to 13 N-m (115 lb in).

4. Connect the door latch electrical connector (1).

Important: Attach the door handle rod retaining clip (1) by pressing clip together over door handle rod until an audible click is heard.

5. Connect the outside door handle rod (2) to the door handle rod retaining clip (1).
6. Inspect for the correct operation of the door handle and door latch.

Important: Firmly press the water deflector where adhesive is applied to make sure of a water tight bond.

7. Install the rear half of the water deflector to the door panel.
8. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement.