For 1990-2009 cars

### Removal procedure

1. Remove the centre console end panel. Refer to Center Console End Panel Replacement.
2. Open the armrest assembly to 180° to the horizontal position.
3. Using a suitable tool spread the centre console retaining lugs (2) away from the armrest assembly arms (3) and remove the armrest assembly (4) from the centre console (1).

### Installation Procedure

1. Align the armrest assembly (4) with centre console assembly (1).
2. Install the armrest assembly arms (3) by firmly inserting it into the centre console retaining lugs (2) listen for an audible click to confirm fitting.
3. Close the armrest assembly (4).
4. Install the centre console end panel. Refer to Center Console End Panel Replacement.