For 1990-2009 cars

1. Install the oil pan baffle (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the oil pan baffle to oil pan retaining bolts (1).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Install a NEW oil suction pipe seal (1) onto the oil suction pipe (2).
4. Install the oil suction pipe (2).
5. Install the oil suction pipe to oil pan retaining bolts (1).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

6. Install the oil pan scraper (2).
7. Install the oil pan scraper to oil pan retaining bolts (1).

Tighten
Tighten the oil pan scraper bolts to 10 N·m (89 lb in).

8. Install the oil pan drain plug (2).

Tighten
Tighten the oil pan drain plug to 20 N·m (15 lb ft).

9. Install the oil level sensor (3).
10. Install the oil level sensor to oil pan retaining bolt (1).

Tighten
Tighten the bolt to 10 N·m (89 lb in).