For 1990-2009 cars

## Fluid Pump Cover Cleaning and Inspection 6L80/6L90

Callout | Component Name
--- | ---
Warning: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result.

#### Preliminary Procedure

Clean and inspect all components and machined surfaces.

1 | Pressure Regulator Valve Train
2 | Converter Feed Limit Valve Train
3 | Pressure Relief Ball Valve and Spring
4 | TCC Control Valve and Spring
5 | A/Trans Fluid Pump Locator Pin