For 1990-2009 cars

## Fastener Tightening Specifications Petrol

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Bolt | 9 N·m | 80 lb in
Air Cleaner Bolt | 9 N·m | 80 lb in
Camshaft Position (CMP) Actuator Solenoid Valve to Engine Front Cover Retaining Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor to Engine Front Cover Retaining Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Control Module (ECM) Bracket to chassis Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 22 N·m | 16 lb ft
Evaporative Emission (EVAP) Canister Bolt | 6 N·m | 53 lb in
Fuel Filler Tube Brace Bolt | 9 N·m | 80 lb in
Fuel Filler Tube Hose Clamp | 4 N·m | 31 lb in
Fuel Tank Strap Bolt | 50 N·m | 37 lb ft
Heated Oxygen Sensor (HO2S) | 40 N·m | 30 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Intake Manifold Runner Control Solenoid Bolt | 10 N·m | 89 lb in
Knock Sensor Bolt | 23 N·m | 17 lb ft
MAF Sensor Screw | 4 N·m | 35 lb in
Rear Frame Bolt First pass Second pass | 65 N·m 120 degrees | 48 lb ft
Spark Plugs
Fit New Spark Plug | 20 N·m | 15 lb ft
Refit Existing Spark Plug | 18 N·m | 13 lb ft
Throttle Body Bolts to Upper Intake Manifold Retaining Bolts | 10 N·m | 89 lb in