For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement.
2. Grasp the front lower area of the centre A pillar ventilation trim panel (2) and carefully pull to disengage the retaining clips (1). The left side is shown, the right side is similar.
3. Remove the centre A pillar ventilation trim panel (2) rotating upwards to disengage remaining clips.

### Installation Procedure

1. Align the center A pillar ventilation trim panel (2) to the A pillar and correctly locate the upper clips (1).
2. Install the center A pillar ventilation trim panel (2) to the A pillar by engaging the retaining clips (1).
3. Ensure all clips are installed correctly.
4. Install the instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement.