For 1990-2009 cars

Name | 5L40-E
--- | ---
RPO Codes | M82, MX5
Vehicle Platform (Engine/Transmission) Usage | D, E, Y
Tranmission Drive | Rear Wheel Drive
1st Gear Ratio | 3.42:1
2nd Gear Ratio | 2.21:1
3rd Gear Ratio | 1.60:1
4th Gear Ratio | 1.00:1
5th Gear Ratio | 0.75:1
Reverse Ratio | 3.03:1
Torque Converter Size (Diameter of Torque Converter Turbine) | 245 mm / 258 mm
Pressure Taps | Line Pressure
Transmission Fluid Type | Dexron™ VI
Transmission Fluid Capacity (Approximate) | Bottom Pan Removal Complete Overhaul: Dry 8.5 L (9.0 qt)
Transmission Type: 5 | Five Forward Gears
Transmission Type: L | Longitude Mount
Transmission Type: 40 | Product Series
Transmission Type: E | Electronic Controls
Position Quadrant | P, R, N, D
Case Material | Die Cast Aluminium
Transmission Weight Dry | (161.0 lb.) 73 kg
Transmission Net Weight | (177.0 lb.) 80.5 kg
Maximum Trailer Towing Capacity | Domestic: 2100 kg Export: 2100 kg
Maximum Gross Vehicle Weight | 3,500 kg (7,716 lbs)