For 1990-2009 cars

Table 1: | Remote Control Door Lock Receiver Scan Tool Data Parameters
Table 2: | Remote Control Door Lock Receiver Scan Tool Output Controls

#### Remote Control Door Lock Receiver Scan Tool Data Parameters

Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Operating Conditions: Ignition ON
Fob 1 Battery | -- | OK | The scan tool displays OK or Low. This is the state of the Fob 1 battery.
Fob 1 Function | -- | None | The scan tool displays None. This is the state of the Fob 1 command as monitored by the RCDLR.
Fob 1 Programmed | -- | Yes | The scan tool displays Yes or No. Yes is displayed if the Fob 1 is programmed into the RCDLR.
Fob 2 Battery | -- | OK | The scan tool displays OK or Low. This is the state of the Fob 2 battery.
Fob 2 Function | -- | None | The scan tool displays None. This is the state of the Fob 2 command as monitored by the RCDLR.
Fob 2 Programmed | -- | Yes | The scan tool displays Yes or No. Yes is displayed if the Fob 2 is programmed into the RCDLR.
Fob 3 Battery | -- | OK | The scan tool displays OK or Low. This is the state of the Fob 3 battery.
Fob 3 Function | -- | None | The scan tool displays None. This is the state of the Fob 3 command as monitored by the RCDLR.
Fob 3 Programmed | -- | Yes | The scan tool displays Yes or No. Yes is displayed if the Fob 3 is programmed into the RCDLR.
Fob 4 Battery | -- | OK | The scan tool displays OK or Low. This is the state of the Fob 4 battery.
Fob 4 Function | -- | None | The scan tool displays None. This is the state of the Fob 4 command as monitored by the RCDLR.
Fob 4 Programmed | -- | Yes | The scan tool displays Yes or No. Yes is displayed if the Fob 4 is programmed into the RCDLR.
Last Fob Used | -- | Varies | The scan tool displays None, Fob 1, Fob 2, Fob 3, Fob 4 or Fob 5. This was the last Fob used, as monitored by the RCDLR.
LF Pressure Sensor Mode | -- | Varies | The scan tool displays Learn, Re-measure, Off, Stationary, Wake up, and Learn. This is the state of the left front pressure sensor.
LF Pressure Status | -- | Normal | The scan tool displays Unknown, Normal, Low. This is the state of the left front tire pressure.
LF Tire Press. Sensor Status | -- | Normal | The scan tool displays Normal Mode, Fault or Low Battery. This is the state of the left front tire pressure sensor.
LF Tire Press. Sensor Battery Status | -- | OK | The scan tool displays OK or Low Battery This is the state of the left front tire pressure sensor battery
LF Tire Pressure | -- | kPa (psi) | This displays kPa (psi). This is the amount of pressure in the left front tire.
LR Pressure Sensor Mode | -- | Varies | The scan tool displays Learn, Re-measure, Off, Stationary, Wake up, and Learn. This is the state of the left rear pressure sensor.
LR Pressure Status | -- | Normal | The scan tool displays Unknown, Normal, Low, Low. This is the state of the left rear tire pressure.
LR Tire Press. Sensor Status | -- | Normal | The scan tool displays Normal Mode, Fault or Low Battery. This is the state of the left rear tire pressure sensor.
LR Tire Pressure | -- | kPa (psi) | This displays kPa (psi). This is the amount of pressure in the left rear tire.
LR Tire Press. Sensor Battery Status | -- | OK | The scan tool displays OK or Low Battery This is the state of the left rear tire pressure sensor battery
Rear Placard | -- | Counts | This displays Counts.
Front Placard | -- | Counts | This displays Counts.
RF Pressure Sensor Mode | -- | Varies | The scan tool displays Learn, Re-measure, Off, Stationary, Wake up, and Learn. This is the state of the right front pressure sensor.
RF Pressure Status | -- | Normal | The scan tool displays Unknown, Normal, Low, Low. This is the state of the right front tire pressure.
RF Tire Press. Sensor Status | -- | Normal Mode | The scan tool displays Normal Mode, Fault or Low Battery. This is the state of the right front tire pressure sensor.
RF Tire Pressure | -- | kPa (psi) | This displays kPa (psi). This is the amount of pressure in the right front tire.
RF Tire Press. Sensor Battery Status | -- | OK | The scan tool displays OK or Low Battery This is the state of the right front tire pressure sensor battery
RR Pressure Sensor Mode | -- | Varies | The scan tool displays Learn, Re-measure, Off, Stationary, Wake up, and Learn. This is the state of the right rear pressure sensor.
RR Pressure Status | -- | Normal | The scan tool displays Unknown, Normal, Low, Low. This is the state of the right rear tire pressure.
RR Tire Press. Sensor Status | -- | Normal | The scan tool displays Normal Mode, Fault or Low Battery. This is the state of the right rear tire pressure sensor.
RR Tire Pressure | -- | kPa (psi) | This displays kPa (psi). This is the amount of pressure in the right rear tire.
RR Tire Press. Sensor Battery Status | -- | OK | The scan tool displays OK or Low Battery This is the state of the right rear tire pressure sensor battery
Selected Front Tire Type | -- | Varies | The scan tool displays, P-Metric (S). This is the type of rear tires used on the vehicle.
Selected Rear Tire Type | -- | Varies | The scan tool displays, P-Metric (S). This is the type of rear tires used on the vehicle.
Tire Pressure Monitoring (TPM) System Enabled | -- | Yes | The scan tool displays Yes or No. Yes is displayed if the TPM system is enabled.
TPM Indicator Message | -- | On | The scan tool displays On or Off. On is displayed if the TPM Indicator Message is visible.
Off
Learn in Progress | -- | Yes | The scan tool displays Yes or No. Yes is displayed if the TPM is in learn mode.
No

#### Remote Control Door Lock Receiver Scan Tool Output Controls

Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Key Fob Button Test | Special Functions | This program will erase all key fobs from memory and then begin reprogramming