For 1990-2009 cars

### Removal Procedure

Caution: Refer to Protective Goggles and Glove Caution in the Preface section.

Important: When a suitable hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Install a suitable hood brace to the vehicle.

Important: The secondary hood latch retaining pin (1) is a single use part only. It must be discarded after removal.

2. Remove the secondary hood latch retaining pin (1) from the secondary hood latch (2).

Discard the pin.

3. Remove the secondary hood latch (2) from the vehicle.

### Installation Procedure

1. Install the secondary hood latch (2) to the vehicle.
2. Install a NEW secondary hood latch retaining pin (1) to the secondary hood latch.
3. Crimp the exposed end of the secondary hood latch retaining pin (1) to make sure the retaining pin is secure.