For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement.
3. Remove the throttle body electrical connector (1) from the throttle body.
4. Remove the the throttle body bolts to upper intake manifold retaining bolts (1)
5. Remove the throttle body and gasket from the vehicle.

### Installation Procedure

1. Carefully clean the throttle body mounting surfaces of any gasket and/or sealing material.
2. Install the throttle body and NEW gasket to the vehicle

Notice: Refer to Fastener Notice in the Preface section.

3. Install the throttle body bolts to upper intake manifold retaining bolts (1).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install the throttle body electrical connector (1) to the throttle body.
5. Install the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement.
6. Perform the idle learn procedure. Refer to Idle Learn
7. Use the scan tool to clear all DTCs.