For 1990-2009 cars

## Radiator Outlet Hose Replacement 3.6L Engine

### Removal Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .

Caution: Refer to Safety Glasses Caution in the Preface section.

Important: If outlet hose (1) is not being replaced leave retaining clamp (2) attached to outlet hose.

2. Release the retaining hose clamp (1) and remove the outlet hose (2).

Caution: Refer to Vehicle Lifting Caution in the Preface section.

3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Remove the air deflector. Refer to Front Air Deflector Replacement .

Important: If outlet hose (1) is not being replaced leave retaining clamp (2) attached to hose.

Important: Access to the outlet hose is restricted, removal of the cooling fan's will aid access. Refer to Cooling Fan and Shroud Replacement .

5. Remove the outlet hose (1) by releasing the retaining hose clamp (2)

### Installation Procedure

Caution: Refer to Installing Hoses without Twists or Bends Notice in the Preface section.

1. Install the outlet hose (1) and secure it with the retaining hose clamp (2).
2. Install the air deflector. Refer to Front Air Deflector Replacement .
3. Lower the vehicle.

Caution: Refer to Safety Glasses Caution in the Preface section.

4. Secure the outlet hose (2) by opening the retaining hose clamp (1) and sliding it over the hose (2).
5. Install the radiator air baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement .
6. Fill the cooling system. Refer to Cooling System Draining and Filling .
7. Inspect cooling system for leaks.