For 1990-2009 cars

### Removal Procedure - Door Handle Cable

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Remove the door latch. Refer to Front Side Door Latch Replacement.
4. Disconnect the door handle cable (2) from the door latch (1).

### Installation Procedure - Door Handle Cable

1. Connect the door handle cable (2) to the door latch (1).
2. Install the door latch. Refer to Front Side Door Latch Replacement.
3. Install the water deflector. Refer to Front Side Door Water Deflector Replacement.
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement.

### Removal Procedure - Lock Cable

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Remove the door latch. Refer to Front Side Door Latch Replacement.
4. Disconnect the door lock cable (2) from the door latch (1).

### Installation Procedure - Lock Cable

1. Connect the lock handle cable (2) to the door latch (1).
2. Install the door latch. Refer to Front Side Door Latch Replacement.
3. Install the water deflector. Refer to Front Side Door Water Deflector Replacement.
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement.