For 1990-2009 cars

Callout | Component Name
--- | ---
Note: Do not remove the park pawl or park pawl spring. The park pawl and park pawl spring are not serviceable components.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the transmission fluid pan. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement.
3. Remove the manual shaft detent assembly roller. Refer to Control Valve Lower Body and Upper Body Replacement

1 | Manual Shaft Detent Lever Hub Pin Tip

• | Discard the pin. Replace with NEW pin.

• | "Walk" the pin out using side cutters.

2 | Manual Shift Shaft Pin Tip

• | Discard the pin. Replace with NEW pin.

• | "Walk" the pin out using side cutters.

3 | Manual Shift Shaft
4 | Manual Shaft Detent Lever Assembly
5 | Park Pawl Actuator Assembly
6 | Park Pawl Actuator Guide Pin Tip

• | Discard the pin. Replace with NEW pin.

• | "Walk" the pin out using side cutters.

7 | Park Pawl Actuator Guide
8 | Park Pawl Actuator Guide (O-Ring) Seals (Qty: 2) Tip Discard the seals. Replace with NEW seals.