For 1990-2009 cars

## Floor Rear Air Outlet Duct Replacement - Left Side LHD

### Removal Procedure

1. Remove the front carpet. Refer to Front Floor Panel Carpet Replacement.
2. Remove centre console. Refer to Front Floor Console Replacement.
3. Remove the retaining pins (1) from the duct (2) .
4. Remove the duct (1) from floor.
5. Disconnect the duct (1) from the module.

### Installation Procedure

1. Install the duct to the module (1).
2. Install the duct to the floor.
3. Install the retaining pin (1) to the duct (2) .
4. Install the centre console. Refer to Front Floor Console Replacement.
5. Install the front carpet. Refer to Front Floor Panel Carpet Replacement.