For 1990-2009 cars

#### Tools Required

J 44827 Transmission Cooler Quick Disconnect

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front air deflector. Refer to Front Air Deflector Replacement .
3. Place an oil drain pan under the transmission fluid cooler pipes (1&2) near the radiator.
4. Disconnect the transmission fluid cooler pipes from the transmission fluid cooler by using the J 44827 .
5. Remove the transmission fluid cooler pipes bracket retaining bolt.
6. Remove the transmission fluid cooler pipes retaining bolt.
7. Remove the transmission fluid cooler pipes.
8. Remove and discard the O-rings. Do not reuse the O-rings.

### Installation Procedure

1. Install the transmission fluid cooler pipe.
2. Connect the transmission fluid cooler pipes (1&2) to the transmission fluid cooler using the following steps:

2.1. | Push the transmission fluid cooler pipes into the quick connect fitting, until a "audible click" is heard.

2.2. | Tug gently on the transmission cooler pipes to make sure the trans cooler pipes are fully connected.

3. Install NEW sealing washers over the transmission fluid cooler pipes.
4. Install the transmission fluid cooler pipes into the transmission.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the transmission fluid cooler pipe retaining bolt.

Tighten
Tighten the transmission fluid cooler pipe retainer bolt to 25 N·m (18 lb. ft).

6. Install the transmission fluid cooler pipes bracket retaining bolt.

Tighten
Tighten the transmission fluid cooler pipes bracket bolt to 50 N·m (37 lb. ft).

7. Install the front air deflector. Refer to Front Air Deflector Replacement .
8. Lower the vehicle.
9. Inspect the transmission fluid level. Refer to Transmission Fluid Check .
10. Inspect for fluid leaks.