For 1990-2009 cars

## Instrument Panel Insulator Panel Replacement - Right Side LHD

### Removal Procedure

1. Grasp the instrument panel (I/P) insulator panel (1) and carefully pull downward to disengage the retaining clips.
2. Remove the courtesy lamp socket assembly (2) from the I/P insulator panel by turning the socket counter-clockwise.
3. Remove the I/P insulator panel (1).

### Installation Procedure

1. Align the I/P insulator panel (1) to the I/P.
2. Install the courtesy lamp socket assembly (2) to the I/P insulator panel (1).

Important: Listen for audible clicks when fitting the I/P insulator panel to confirm correct fitment.

3. Attach the I/P insulator panel (1) to the I/P by engaging the retaining clips.