For 1990-2009 cars

## Coolant Recovery Reservoir Pipe Replacement 3.6L Engine

### Removal Procedure

1. Remove the radiator air baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement in Body Front End.
2. Detach the coolant recovery hose (2) from the radiator outlet pipe (1).
3. Remove the coolant recovery hose (2) from the coolant recovery reservoir filler neck (1).
4. Detach and remove the coolant recovery reservoir hose (1) from the coolant recovery reservoir retaining locks (3) located on the radiator (2).

### Installation Procedure

1. Install the coolant recovery reservoir hose (2) into the coolant recovery reservoir filler neck (1).
2. Attach the coolant recovery reservoir hose (1) into the coolant recovery reservoir retaining locks (3) located on the radiator (2).
3. Attach the coolant recovery reservoir hose (2) to the radiator outlet pipe (1).
4. Install the radiator air baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement in Body Front End.
5. Check the coolant level. Refer to Cooling System Draining and Filling.