For 1990-2009 cars

#### Tools Required

AU-533 Fuel Line Quick Connect Separator

### Removal Procedure

Caution: Refer to Gasoline/Gasoline Vapors Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .
2. Blow dirt out of the fitting using compressed air.
3. Install the quick connect tool over the quick connect fitting (1).
4. Pull the connection apart.
5. Using a clean shop towel, wipe off the male pipe end
6. Inspect both ends of the fitting for dirt and burrs.
7. Clean or replace the components as required.

### Installation Procedure

Caution: In order to reduce the risk of fire and personal injury, before connecting fuel pipe fittings, always apply a few drops of clean engine oil to the male pipe ends.

This will ensure proper reconnection and prevent a possible fuel leak. During normal operation, the O-rings located in the female connector will swell and may prevent proper reconnection if not lubricated.
1. Apply a few drops of clean engine oil to the male pipe end.
2. Push both sides (1 & 2) of the quick-connect fitting together to cause the retaining tabs/fingers to snap into place.
3. Pull on both sides of the quick-connect fitting (1) to make sure the connection is secure.
4. Inspect for leaks using the following procedure:

4.1. | Turn the ignition ON, with the engine OFF for 2 seconds.

4.2. | Turn the ignition OFF, for 10 seconds.

4.3. | Turn the ignition ON, with the engine OFF for 2 seconds.

4.4. | Turn the ignition OFF.

4.5. | Inspect for leaks.