For 1990-2009 cars

## Secondary Driver Information Display Replacement Base

### Removal Procedure

1. Remove the instrument panel (I/P) upper trim panel assembly. Refer to Instrument Panel Center Trim Panel Replacement.
2. Remove the secondary information centre (SIC) display to I/P upper trim panel assembly retaining screws (3).
3. Remove the SIC display (2) from the I/P upper trim panel assembly (1).

### Installation Procedure

1. Install the SIC display (2) to the I/P upper trim panel assembly (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the SIC display to I/P upper trim panel assembly retaining screws (3).

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the I/P upper trim panel assembly. Refer to Instrument Panel Center Trim Panel Replacement.
4. For programming and setup, refer to Control Module References.