For 1990-2009 cars

#### Tools Required

• | EN 46106 Flywheel Holding Tool

• | 303-642 Harmonic Balancer Puller

1. Install the EN 46106 (1) through the starter mounting hole.
2. Remove the crankshaft balancer to crankshaft retaining bolt (1).
3. Install the 303-642 (1).

Important: Remove the crankshaft balancer off by tightening the center bolt on the 303-642 (1) until the crankshaft balancer (2) is removed from the crankshaft.

4. Remove the crankshaft balancer (2).
5. Remove the 303-642 (1) from the crankshaft balancer.