For 1990-2009 cars

## Rear Seat Belt Replacement LHD

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement.
2. Remove the rear seat back. Refer to Rear Seat Back Replacement.
3. Remove the upper rear quarter trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Remove the bolt (1) attaching the seat belt lower anchor (2) to the vehicle
5. Remove the rear seat belt guide bolt assembly (1).
6. Remove the rear seat belt retractor bolt (2).
7. Lift the retractor (1) in a upwards direction and tilt on a 30 degree angle making sure that the locking tab is clear

### Installation Procedure

1. Replace the rear seat belt retractor assembly (1) and rear seat belt retractor bolt (2) .

Tighten
Tighten the intermediate bolt (2) to 43 N·m (31 lb ft).

2. Replace the rear seat belt guide bolt assembly (1).

Tighten
Tighten the rear seat belt guide mounting bolt (4) to 43 N·m (32 lb ft).

3. Replace the upper rear quarter trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Replace the bolt (1) attaching the seat belt lower anchor (2) to the vehicle

Important: Make Sure the seat belt lower anchor is parallel to vehicle centreline as shown.

Tighten
Tighten the seat belt lower anchor mounting bolt (1) to 43 N·m (31 lb ft).

5. Replace the rear seat cushion. Refer to Rear Seat Cushion Replacement.
6. Replace the rear seat back. Refer to Rear Seat Back Replacement.