For 1990-2009 cars

### Removal Procedure

1. Remove the defrost grille. Refer to Defroster Grille Replacement.
2. Detach the sunload sensor (2) electrical connector retaining pin (3).
3. Remove the sunload sensor electrical connector (3).

### Installation Procedure

1. Install the sunload electrical connector (3).
2. Attach the sunload electrical connecter retaining pin (1).
3. Install the defrost grille. Refer to Defroster Grille Replacement.
4. Test the sunload sensor for the correct operation.