For 1990-2009 cars

## Rear Compartment Lid Applique Replacement LWB

### Removal Procedure

1. Support the rear compartment lid with a suitable brace.
2. Remove the rear compartment lid moulding to rear compartment lid retaining nuts (3).
3. Use a suitable tool to carefully pry the rear compartment lid moulding (1) from the rear compartment lid.

Important: The rear compartment lid moulding retaining clips are a single use part.

4. Remove the rear compartment lid retaining clips (2) from the rear compartment lid moulding (1) and discard.

Discard the retaining clips.

### Installation Procedure

1. Install NEW rear compartment lid retaining clips (2) to the rear compartment lid moulding (1).
2. Align the rear compartment lid moulding datum pin (2) to the rear compartment lid datum hole (1).
3. Firmly press the rear compartment lid moulding to the compartment lid rear.
4. Install the rear compartment lid moulding (1) to rear compartment lid retaining nuts (2).

Tighten
Tighten the nuts to 2 N·m (18 lb in).

5. Remove the suitable brace from the vehicle.