For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Caution: Refer to Exhaust Service Caution in the Preface section.

2. Remove the right rear muffler assembly. Refer to Exhaust Muffler Replacement - Right Side.
3. Remove the right exhaust muffler heat shield to body retaining bolts (1).
4. Remove the right exhaust muffler heat shield (2).

### Installation Procedure

1. Position the right exhaust muffler heat shield (2) to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the right exhaust muffler heat shield to body retaining bolts (1).

Tighten
Tighten the bolts to 4 N·m (35 lb in).

3. Install the right rear muffler assembly. Refer to Exhaust Muffler Replacement - Right Side.
4. Lower the vehicle to the ground.