For 1990-2009 cars

### Removal Procedure

1. Remove the rear sill trim panel. Refer to Door Sill Plate Replacement.
2. Remove the centre pillar lower trim. Refer to Center Pillar Lower Trim Panel Replacement.
3. Remove the trim panel - upper centre pillar, on both sides. Refer to Center Pillar Upper Trim Panel Replacement.
4. Remove the trim panel - rear quarter lower. Refer to Quarter Lower Rear Trim Panel Replacement.
5. Remove the trim panel - rear quarter upper. Refer to Quarter Upper Trim Panel Replacement.
6. Starting from the centre sill point (3) carefully remove the rear door weatherstrip (2) from the body panel door opening (1).

### Installation Procedure

Important: Make sure the lip of the weatherstrip sits over the trim panels.

Important: Make sure the weatherstrip does not short cut the corners and foul the door trim.

1. Starting at the centre sill point (2) install the rear door weatherstrip (3) to the body panel door opening (1).
2. Install the trim panel - rear quarter upper. Refer to Quarter Upper Trim Panel Replacement.
3. Install the trim panel - rear quarter lower. Refer to Quarter Lower Rear Trim Panel Replacement.
4. Install the trim panel - upper centre pillar, on both sides. Refer to Center Pillar Upper Trim Panel Replacement.
5. Install the centre pillar lower trim. Refer to Center Pillar Lower Trim Panel Replacement.
6. Install the rear sill trim panel. Refer to Door Sill Plate Replacement.