For 1990-2009 cars

1. Install the NEW overdrive clutch fluid passage sleeve (39) into the case.
2. Install the NEW centre support fluid passage sleeve (38) into the case.
3. Install the control valve body accumulator assembly (47) onto the case.
4. Install the detent lever spring (52) onto the case.
5. Install the control valve body retaining bolts (53) into the case and hand tighten.
6. Install the control valve body accumulator assembly bolts (49, 51) into the case and hand tighten.

Notice: Refer to Fastener Notice in the Preface section.

7. Tighten the control valve body accumulator retaining bolts in sequence.

Tighten
Tighten the control valve body accumulator bolts to 11 N·m (8 lb. ft).

8. Install a 0.8 mm spacer (1) between the shift shaft detent lever (600) and the shift shaft detent assembly (52).
9. Tighten the detent assemby bolts (53).

Tighten
Tighten the control valve body bolts (53) to 11 N·m (8 lb. ft).

10. Remove the spacer (1).