For 1990-2009 cars

## Headlamp Switch Replacement LHD

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable from the battery. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove headlamp switch (1) from I/P trim pad by gently prizing the switch assembly from the IP crashpad.
3. Disconnect the headlamp switch electrical connector.
4. Remove the headlamp switch.

### Installation Procedure

1. Connect the headlamp switch electrical connector.
2. Install the headlamp switch (1) to the I/P trim pad.
3. Connect the battery ground cable to the battery. Refer to Battery Negative Cable Disconnection and Connection.
4. Check all vehicle lights for correct operation.