For 1990-2009 cars

## Front Bumper Fascia Insert Replacement LWB SWB

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.
3. Carefully pry the front bumper fascia insert retaining tabs (1) from the front bumper fascia.
4. Remove the front bumper fascia insert from the front bumper fascia.

### Installation Procedure

1. Install the front bumper fascia insert to the front bumper fascia.
2. Firmly press the front bumper fascia insert retaining tabs (1) into the front bumper fascia.
3. Install the front air deflector. Refer to Front Air Deflector Replacement.
4. Lower the vehicle.