For 1990-2009 cars

### Removal Procedure

1. Pull the lower corners of the front seat-back trim (3) away from the seat (1) disengaging the two retaining clips (2).
2. While holding the lower section of the rear trim cover (2) out, pull the cover down to release the two upper retaining lugs (1).
3. Remove the rear trim cover (2).

### Installation Procedure

Notice: Refer to General Repair Instructions in the Preface section.

1. Align the two upper retaining lugs (1) with the seat-back.
2. Push the front seat-back rear trim cover (2) up and in at the lower edge to engage the two lower retaining clips.