For 1990-2009 cars

Important: Make sure all mating surfaces are clean and free of grease.

1. Using a water sealant install the water pump and gasket to front engine cover.
2. Make sure all retaining bolts are clean and free of debris.
3. Install the water pump (1) and NEW gasket (2).

Notice: Refer to Fastener Notice in the Preface section.

4. Install the water pump to engine front cover retaining bolts (3).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

5. Install the water pump pulley (2) to the water pump (3)
6. Install the water pump pulley to water pump retaining bolts (1).

Tighten
Tighten the bolts to 10 N·m (89 lb in).