For 1990-2009 cars

### Tools Required

• | EN 46106 Flywheel Holding Tool.

• | J 45059 Angle Meter.

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement .

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the starter motor. Refer to Starter Motor Replacement .
4. Install the EN 46106 (1) through the starter mounting hole.
5. Lower the vehicle.
6. Remove the front air deflector. Refer to Front Air Deflector Replacement .
7. Remove the crankshaft balancer. Refer to Crankshaft Balancer Removal .

### Installation Procedure

1. Install the crankshaft balancer. Refer to Crankshaft Balancer Installation .
2. Install the front air deflector. Refer to Front Air Deflector Replacement .
3. Raise the vehicle.
4. Remove EN 46106 (1) from the starter mounting hole.
5. Remove the starter motor. Refer to Starter Motor Replacement .
6. Install the drive belt. Refer to Drive Belt Replacement .