For 1990-2009 cars

### Removal Procedure

1. Remove the applicable camshaft(s). Refer to Camshaft Replacement - Right Side.
2. Remove the rocker arms. Refer to Valve Rocker Arm Removal - Right Side.
3. Clean and inspect the camshaft(s) and the rocker arm(s). Repair or replace as necessary. Refer to Camshaft Cleaning and Inspection and Valve Lifters Cleaning and Inspection.

### Installation Procedure

1. Install the rocker arms. Refer to Valve Rocker Arm Installation - Right Side.
2. Install the applicable camshaft(s). Refer to Camshaft Installation - Right Side.