For 1990-2009 cars

## Cylinder Head Removal - Right Side LLT

1. Remove the right cylinder head bolts.
2. Remove the right cylinder head.
3. Remove and discard the right cylinder head gasket.

## Cylinder Head Removal - Right Side LY7

1. Remove the right bank cylinder head to cylinder block retaining bolts (1).
2. Remove the right bank cylinder head (2).
3. Remove and discard the right cylinder head gasket (1).