For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) upper trim pad. Refer to Instrument Panel Upper Trim Pad Replacement.
2. Remove the air outlet duct to I/P upper trim pad retaining screws (2).
3. Remove the air outlet duct (1) from the I/P upper trim pad (3).

### Installation Procedure

1. Install the air outlet duct (1) to the instrument panel (I/P) upper trim pad (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the air outlet duct to I/P upper trim pad retaining screws (2).

Tighten
Tighten the screws to 2 N·m(18lb in).

3. Install the I/P upper trim pad. Refer to Instrument Panel Upper Trim Pad Replacement.