For 1990-2009 cars

## Rear Bumper Fascia Insert Replacement LWB

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
3. Remove the rear bumper fascia moulding to rear bumper fascia retaining scrivets (1).
4. Disengage the retaining tabs (1) from the rear bumper fascia (2).
5. Remove the rear bumper fascia moulding (3) from the rear bumper fascia (2).

### Installation Procedure

1. Install the rear bumper fascia moulding (3) to the rear bumper fascia (2).
2. Firmly press the retaining tabs (1) into the rear bumper fascia (2).
3. Install the rear bumper fascia moulding to rear bumper fascia retaining scrivets (1).
4. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
5. Lower the vehicle.